NFIA Board Class Rule Update 2023-03-08

Class Rules changes, immediate introduction.

1.61	If a yacht is to be re-measured (see rule 1.64 below) this shall be carried out in accordance with the rules in force at the time the yacht's original measurement certificate was issued, except that spars, rigging, sail and weight shall be measured in accordance with the current class rules.


9.14  	The class insignia (letter F), national letters and sail numbers shall be placed as laid down in current
 	WORLD SAILING Racing Rules, Appendix G.
 
  	Letters and numbers shall not be less than the following dimensions:
  	Height	300 mm
  	Width	200 mm (excluding number 1 and letter I)
  	Thickness	min 40 mm - max 50 mm
  	Space between adjoining letters and numbers  60 mm

10.    WEIGHT OF NORDIC FOLKBOAT

10.10	The weight of the boat shall not be less than 1930 kg. weighed complete with floorboards, pumps, seats, and all fittings normally used on board whilst racing, together with the following: Mast and boom ( without whisker pole and /or spinnaker pole ) with all their fittings, standing rigging, halyards and sheets for mainsail.
The material of the mast and boom must be stated in the boat's measurement certificate. The equipment included in the weight of not less than 1930kg shall not thereafter be removed whilst racing and shall be in its normal position whilst racing; e.g. the helmsman’s seat.


10.20 	If the boat is found to be underweight, corrector weights of any material having a specific gravity no greater than that of lead, totalling not more than 30 kg. shall be fastened to the hull as described in 10.20.1, 10.20.2 and 10.20.3 below.


10.20.1	Boats built before 01.01 2002 are permitted to have corrector weights to bring the keel weight up to a maximum of 1050 kg weight in accordance with rule 4.20. The actual keel weight shall be confirmed by the measurement certificate. Corrector weights shall be mounted in the bilge at stations 8, 5, 9, 7, 10 and 6 the sequence is mandatory, in pieces up to 10 kg. Pieces may be split if lifting eyes are in the way.

10.20.2	Remaining hull correctors shall be placed:
-To 40 % at not less than 3.40 m aft of the forward face of the mast, no deeper than 578 mm below a line joining the two sheer lines.
-To 60% not less than 0.25 m and not more than 0.60 m forward of the forward face of the mast, no deeper than 844 mm below a line joining the two sheer lines.
The corrector weight may be divided and placed off the centerline. 

10.20.3	Boats built 01.01.2002 or later and found to be underweight are permitted to have hull correctors only totaling not more than 30 kg and mounted as described in 10.20.2 above.
Keel correctors and additional correctors are not permitted for boats built 01.01.2002 or later.
(Note: Grandfathers law applies to boats built before 1’ January 2000 – see rule 1.61)

10.30	The correctors shall be fixed by such means that they cannot be removed without the use of tools.

10.40	The weight and position of all corrector weights shall be entered on the yacht's measurement certificate.

Class Rules Clarification

12.20	A rod kick that is adjusted with a trimming system consisting of blocks and rope with
an integrated passive gas spring that pushes out the kick rod, is not to be seen as an
entire hydraulic or pneumatic system for trimming. This kind of trimming system is not
against CR 12.20.


[bookmark: _bookmark1][bookmark: _bookmark0]9.21/9.15	In cases where the boom's groove runs all the way up to the front edge of the boom, it is permitted to end the continuous bolt rope up to 120mm before the tack measurement point 1. The same applies if the boom’s groove goes up to or past the boom point, it is permitted to end the continuous bolt rope up to 120mm before the clew measurement point 1. This does not contradict the purpose of rule CR 9.15 or CR 9.21

[bookmark: _bookmark2][bookmark: _bookmark3]1 As defined in World Sailing Equipment Rules of Sailing Part 2 Section G4





